**Data Set #1:**

<http://gstore.unm.edu/apps/rgis/datasets/b257a7e4-4c0d-4937-9edf-e3ffb0d5e943/metadata/FGDC-STD-001-1998.html>

**File name:**

halbuqshp.zip

**Name:**

Albuquerque 1:100000 Quad Hydrography DLGs

**Dataset file names:**

halbuq\_2.dbf

halbuq\_2.prj

halbuq\_2.sbn

halbuq\_2.sbx

halbuq\_2.shp

halbuq\_2.shp.xml

halbuq\_2.shx

**Description:**

This file contains digital line graph representations of hydrographic features in and near Albuquerque, New Mexico at a scale of 1:100,000 digitized from a USGS quadrangle at a resolution of 0.001 inches.

**Bounding Box:**

***West Bounding Coordinate***-107.000023

***East Bounding Coordinate***-106.000031

***North Bounding Coordinate***35.500031

***South Bounding Coordinate***34.999962

**Spatial Reference Information:**

***Spatial Reference***

***Name***North American Datum of 1927

***Code***EPSG:4267

***URL***http://www.epsg-registry.org/export.htm?gml=urn:ogc:def:crs:EPSG::4267

***Spatial Reference***

***Name***Clarke 1866

***Code***EPSG:7008

***URL***http://www.epsg-registry.org/export.htm?gml=urn:ogc:def:ellipsoid:EPSG::7008

***Spatial Reference***

***Name***National Geodetic Vertical Datum of 1929

***Code***EPSG:5102

***URL***http://www.epsg-registry.org/export.htm?gml=urn:ogc:def:datum:EPSG::5102

**Data Set #2:**

<http://gstore.unm.edu/apps/rgis/datasets/2f4ccda4-a76e-4df0-849e-ee51dbfec492/metadata/FGDC-STD-001-1998.html>

**File:**

RDSGPS2012v1.zip

**Name:**

New Mexico GPS Roads

**Files in dataset:**

RDSGPS2012v1.dbf

RDSGPS2012v1.pj

RDSGPS2012v1.sbn

RDSGPS2012v1.sbx

RDSGPS2012v1.shp

RDSGPS2012v1.shp.xml

RDSGPS2012v1.shx

**Description:**

The New Mexico Road system.

**Bounding Box:**

***West Bounding Coordinate***-109.039649

***East Bounding Coordinate***-103.027231

***North Bounding Coordinate***36.977276

***South Bounding Coordinate***31.952345

**Spatial Reference Information**

***Spatial Reference***

***Name***North American Datum of 1983

***Code***EPSG:4269

***URL***http://www.epsg-registry.org/export.htm?gml=urn:ogc:def:crs:EPSG::4269

***Spatial Reference***

***Name***Geodetic Reference System 80

***Code***EPSG:7019

***URL***http://www.epsg-registry.org/export.htm?gml=urn:ogc:def:ellipsoid:EPSG::7019

***Spatial Reference***

***Name***Universal Transverse Mercator, 13

***Code***EPSG:26713

***URL***http://www.epsg-registry.org/export.htm?gml=urn:ogc:def:crs:EPSG::26713

**Data Set 3:**

Name:

Bernalillio\_20ft.zip

Files:

Bernalillo\_20ft.dbf

Bernalillo\_20ft.prj

Bernalillo\_20ft.sbn

Bernalillo\_20ft.sbx

Bernalillo\_20ft.shp.xml

Bernalillo\_20ft.shx

Bernalillo\_20ft.shp

Name:

Bernalillo County 20 ft contours

Description

This dataset shows the elevational change for the county at 20 foot contours. These contours were created from the 2005 enhanced 10m statewide Digital Elevation Model (DEM).

Bounding box:

***Bounding Coordinates***

***West Bounding Coordinate***-107.195982112

***East Bounding Coordinate***-106.148912564

***North Bounding Coordinate***35.23382379

***South Bounding Coordinate***34.8552029696

#### Spatial Reference Information

***Spatial Reference***

***Name***D WGS 1984

***Code***EDAC:Unknown

***URL***http://gstore.unm.edu

***Spatial Reference***

***Name***WGS 1984

***Code***EPSG:4326

***URL***http://www.epsg-registry.org/export.htm?gml=urn:ogc:def:crs:EPSG::4326

***Spatial Reference***

***Name***WGS 1984 UTM Zone 13N

***Code***EPSG:Unknown

***URL***http://gstore.unm.edu/sprefs/EDAC-Unknown